|  |
| --- |
| SERVICING AND REFILLING WAYBILL |

|  |  |  |
| --- | --- | --- |
| CLIENT INFORMATION | | Date : 27/06/18 |
| Company Name :PRUDENTIAL LIFE INSURANCE | Contact Person: | |
| Address;TESANO | Email: | |
|  | Phone: | |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S/N | EXTINGUISHERS | QTY | SERVICING | REFILLING | CO2 REFILL | HORN/HOSE | HEAD | GUAGE | CARTRIDGE |
|  | 6KG D.P | 6 | 6 |  |  |  |  |  |  |
|  | 3KG CO2 | 7 | 7 |  |  | 5 |  |  |  |
|  | 1KG D.P | 3 | 1 | 2 |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| S/N | COMPONENT | MARK | REMARKS |
| 1 | Label is clear and extinguisher type and instructions can be read easily. |  |  |
| 2 | Handle is intact and not bent or broken. |  |  |
| 3 | Pressure gauge is in the green and is not damaged or showing “recharge”. |  |  |
| 4 | Discharge hoses/nozzle is in good shape and not clogged, cracked or broken. |  |  |
| 5 | Safety pin is in place & intact. Nothing else should be used in place of the pin. |  |  |
| 6 | Extinguisher is not rusty, or has any type of corrosion build up. |  |  |
| 7 | Extinguisher was turned upside down at least three times (shaken). |  |  |
| 8 | Pin and Tamper seal are intact. |  |  |
| 9 | Wheel in good working condition (if applicable). |  |  |
| 10 | Wall hanging bracket. |  |  |
| 11 | Safely and neatly packed in vehicle. |  |  |
| 12 | Positioning (on site up to standard). |  |  |

|  |  |
| --- | --- |
| KUO Maintenance Officer: | Sign |
| Dispatched by: | Sign |
| Customer Name: | Sign |